**MSS0811 LAN Port Control Instruction**

**I. LAN Port Control**

**Method A)** When connecting MSS0811 with a router with DHCP features.

The matrix switcher will auto obtain an IP address, so you can scan the device directly by the control software.

**Method B)** When connecting MSS0811 with a PC without DHCP.

Please make sure that MSS0811 and PC are in the same local area network, and set PC’s IP address to "192.168.1.xxx", except MSS0811’s default IP address 192.168.1.215, then press the "scanning" button on control software to scan the device. If the device cannot be found, wait 30s and then scan again.

PS: check the LAN port indicators to see current state of MSS0811.

Yellow indicator blinking --- data is transmitting

Green indicator keeps on --- connect successfully with Ethernet

**II. Seiral Port Control**

1. Connecting MSS0811 with a PC via serial port.

**2. Press the**

